SECURITY ACCESS PROCEDURE

id091400810300

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Body”
  2. Select “Security”

3. Then, select items from the screen menu in the following order.

  1. Select “PATS Function”

4. Select the items to be performed from the following:

  • Program Additional card key
  • Card Key Code Erase and Program
  • Steering Lock Unit Programming
  • Program additional ignition key
  • Ignition Key Code Erase and Program
  • Customer Spare Key Programming Enable
  • Customer Spare Key Programming Disable
  • Parameter Reset

5. The security access begins and the M-MDS displays the “OUT-CODE”.

  Note
  • When “OUT-CODE” is first displayed, turning the ignition switch from the OFF to the ON position 5 times will change the “OUT-CODE”.

6. Input “IN-CODE” corresponding to “OUT-CODE” displayed on the M-MDS screen.

7. If the security access is successful, selected item can be performed.