BONNET ADJUSTMENT

id091000802400

Gap Adjustment

1. Measure the gap between the bonnet and body.

ac9wzw00003000

  Standard clearance

  a: -2.5—2.5 mm {-0.098—0.098 in}
  b: -1.21—1.79 mm {-0.0476—0.0704 in}
  c: -1.2—1.2 mm {-0.04—0.04 in}
  d: -1.5—1.5 mm {-0.059—0.059 in}

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION)

  (2) Cowl grille (See COWL GRILLE REMOVAL/INSTALLATION)

4. Loosen the bonnet hinge installation bolts and adjust the bonnet.

ac9uuw00002441

5. Tighten the bolts.

Height Adjustment

1. Measure the height difference between the bonnet and body.

ac9wzw00003001

  Clearance

  a: 3.2—7.2 mm {0.13—0.28 in}
  b: 2.0—5.0 mm {0.07—0.19 in}
  c: 2.8—5.2 mm {0.11—0.20 in}

2. Turn the stop rubber to adjust.

ac9wzw00001407