HAZARD WARNING SWITCH REMOVAL/INSTALLATION

id091800803000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

3. Remove in hazard warning switch.

ac9uuw00000429

4. Install in the reverse order of removal.