PURGE SOLENOID VALVE REMOVAL/INSTALLATION [MZI-3.7]

id0116d2803500

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove in the order indicated in the table.

ac9wzw00001559

1 | Purge solenoid valve connector
2 | Quick release connector (See QUICK RELEASE CONNECTOR (EMISSION SYSTEM) REMOVAL/INSTALLATION [MZI-3.7].)
3 | Purge solenoid valve

3. Install in the reverse order of removal.