POWER DOOR LOCK SYSTEM OUTLINE

id091400590300

• A door lock switch interlock function has been adopted where all doors are locked/unlocked when the door is locked/unlocked with the door lock switch.
• A door key interlock function has been adopted where all doors are locked/unlocked when the driver’s door is locked/unlocked with the driver’s door key cylinder.
• All doors unlock if the vehicle has a collision. (with collision detection unlock function)