ULTRASONIC SENSOR SHORT-CORD REMOVAL/INSTALLATION

id092200036900

1. Disconnect the negative battery cable.

2. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the rear bumper. (See REAR BUMPER REMOVAL/INSTALLATION.)

4. Remove the rear reflector. (See REAR BUMPER DISASSEMBLY/ASSEMBLY.)

5. Peel off the tape securing the ultrasonic sensor short-cord from the rear bumper.

ac9wzw00002676

6. Disconnect the connector from the ultrasonic sensor.

7. Pull clip A in the direction of the arrow (2) shown in the figure while pressing the tab of clip A in the direction of the arrow (1) shown in the figure, and detach the tab of clip A and rear bumper.

8. Pull clip B in the direction of the arrow (4) shown in the figure while pressing the tab of clip B in the direction of the arrow (3) shown in the figure, detach the tab of clip B and rear bumper, and remove the ultrasonic sensor short-cord.

ac9wzw00002626

9. Install in the reverse order of removal. (See Ultrasonic Sensor Short-cord Installation Note.)

Ultrasonic Sensor Short-cord Installation Note

1. Align the height of the ultrasonic sensor short-cord with the center of the tape adhering position marking on the rear bumper.

ac9wzw00002739

2. Align the tape with the mark of the tape adhering position marking and adhere the ultrasonic sensor short-cord and rear bumper.