ON-BOARD DIAGNOSTIC OUTLINE [INSTRUMENT CLUSTER]

id092200103343

• If a malfunction occurs in the system, a malfunction detection function is equipped to record the malfunction as a DTC. Recorded DTCs can be read by the Mazda Modular Diagnostic System (M-MDS).
• The diagnostic system records the DTC while also storing the control status of the related instrument cluster as freeze frame data.
• An input/output check function has been adopted that examines input signals to the instrument cluster and individual parts via the micro computer built into the instrument cluster.
• A PID/data monitor function is equipped in the instrument cluster.
• When configuring, the odometer (total traveled distance data) data from the previous instrument cluster can be transferred to the new instrument cluster.