FOREWORD [ENTIRE AUDIO SYSTEM]

id0903e2802700

  Note
  • Record all radio programs set by customer prior to the repairs. Set all radio programs and adjust the time after repairs.

No. | Symptom | Possible DTC
--- | --- | ---
Using the M-MDS | Without using M-MDS (On-board diagnostic test mode)
1 | NO.1 AF NOISE OR POP NOISE AT ALL SOURCES (RADIO, CD) [ENTIRE AUDIO SYSTEM] | U3000:09 | 09:Er21
2 | NO.2 AUDIO POWER IS NOT AVAILABLE OR SWITCHED ON OR OFF AUTOMATICALLY [ENTIRE AUDIO SYSTEM] | U3003:16 | 09:Er20
3 | NO.3 NO SOUND FROM ALL SPEAKERS [ENTIRE AUDIO SYSTEM] | U3003:16, U3000:09 | 09:Er20, 09:Er21
4 | NO.4 NO SOUND FROM SOME SPEAKERS [ENTIRE AUDIO SYSTEM] | — | —
5 | NO.5 SOUND BREAK-UP OR POOR SOUND QUALITY [ENTIRE AUDIO SYSTEM] | U3000:09 | 09:Er21
6 | NO.6 VOLUME INCREASES/DECREASES WHILE DRIVING THE VEHICLE [ENTIRE AUDIO SYSTEM] | — | —
7 | NO.7 ALC FUNCTION IS INOPERATIVE [ENTIRE AUDIO SYSTEM] | U0155:00, U0010:88 | 16:Er12
8 | NO.8 AudioPilot®2 FUNCTION IS INOPERATIVE [ENTIRE AUDIO SYSTEM] | U0155:00, U0010:88 | 16:Er12
9 | NO.9 NO AUDIO SYSTEM ILLUMINATION [ENTIRE AUDIO SYSTEM] | U3003:16 | 09:Er20
10 | NO.10 SOUND JUMPS [ENTIRE AUDIO SYSTEM] | B1188:64 | 10:Er07
11 | NO.11 DISPLAY DOES NOT CHANGE TO THE REAR MOUNT CAMERA IMAGE [ENTIRE AUDIO SYSTEM] | — | —

Quick Diagnostic Chart

ac9wzw00002913

ac9wzw00002914