D-PILLAR TRIM REMOVAL/INSTALLATION

id091700802300

1. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (6) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (7) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (8) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (9) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

2. Remove the PLG arm band. (Vehicles with PLG)

ac9wzw00001505

3. Partially peel back the seaming welt.

4. Remove the fasteners.

ac9uuw00000333

5. Detach clips A and pins B by pulling them in the direction of the arrow.

6. Remove the D-pillar trim.

7. Install in the reverse order of removal.