FOG LIGHT SWITCH INSPECTION

id091800812900

Front Fog Light Switch

1. Disconnect the negative battery cable.

2. Remove the lower column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Put aside the upper column cover.

4. Remove the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

5. Verify that continuity between the front fog light switch terminals is as indicated in the table.

ac9wzw00001723

  • If not as indicated in the table, replace the light switch.

  ac9wzw00001724

Front and rear fog light switch

1. Disconnect the negative battery cable.

2. Remove the lower column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Put aside the upper column cover.

4. Remove the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

5. Verify that the continuity between the fog light switch terminals is as indicated in the table.

ac9wzw00001725

  • If not as indicated in the table, replace the light switch.

  ac9wzw00001726