WINDSHIELD WIPER AND WASHER SWITCH INSPECTION

id091900800300

1. Disconnect the negative battery cable.

2. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove the wiper and washer switch. (See WINDSHIELD WIPER AND WASHER SWITCH REMOVAL/INSTALLATION.)

4. Verify that the continuity between the windshield wiper and washer switch is as indicated in the table.

  • If not as indicated in the table, replace the wiper and washer switch. (See WINDSHIELD WIPER AND WASHER SWITCH REMOVAL/INSTALLATION.)

Windshield Wiper And Washer Switch LH Side (Vehicles Without Auto Wiper System)

ac9wzw00001581

ac9wzw00000672

Windshield Wiper And Washer Switch RH Side (Vehicles Without Auto Wiper System)

ac9wzw00001582

ac9uuw00000735

Windshield Wiper And Washer Switch LH Side (Vehicles With Auto Wiper System)

ac9wzw00001583

ac9wzw00000674

ac9wzw00001496

Windshield Wiper And Washer Switch RH Side (Vehicles With Auto Wiper System)

ac9wzw00001584

ac9uuw00000737

ac9wzw00001585