TORQUE CONVERTER CLUTCH (TCC) CONTROL SOLENOID OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3225100

• The TCC control solenoid is installed on the front valve body. Based on engine speed, throttle opening degree signals, input/turbine speed sensor signals and vehicle speed sensor (VSS) signals, it linearly controls TCC hydraulic pressure. Through this, TCC and slip are controlled. As a fail-safe function, if any TCC control solenoid abnormality occurs, the TCM will disable the current to the solenoid.
• The TCC control solenoid is installed on the front valve body. It linearly controls TCC hydraulic pressure based on engine speed, accelerator pedal depressing amount signals, Input/turbine speed sensor signals, and VSS signals. This results in control of TCC. As a fail-safe function, if any abnormality occurs in the TCC control solenoid, then the TCM will shut off the current to the solenoid.

ac9uun00000838