OIL SEAL (OIL PUMP) REPLACEMENT [AY6A-EL, AY6AX-EL]

id0517k3332400

1. Remove the transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

2. Remove the torque converter. (See TORQUE CONVERTER REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

  Caution
  • Do not damage the oil seal.
  • Do not drop the torque converter.

3. Using a tape-wrapped flathead screwdriver, remove the oil seal from the oil pump body.

am6xuw00004216

  Caution
  • Do not to damage the bushing on the oil pump body.

4. Using the SST and a hammer, install the oil seal to the oil pump body.

am6xuw00004217

5. Coat the lip of the oil seal with grease.

6. Install the torque converter. (See TORQUE CONVERTER REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

  Caution
  • Do not damage the oil seal.
  • Do not drop the torque converter.
  • Do not pinch fingers.

7. Install the transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

8. Add ATF. (See AUTOMATIC TRANSAXLE FLUID (ATF) LEVEL ADJUSTMENT [AY6A-EL, AY6AX-EL].)

9. Adjust the ATF level. (See AUTOMATIC TRANSAXLE FLUID (ATF) LEVEL ADJUSTMENT [AY6A-EL, AY6AX-EL].)

10. Perform the “MECHANICAL SYSTEM TEST”. (See MECHANICAL SYSTEM TEST [AY6A-EL, AY6AX-EL].)