DOOR LOCK SWITCH REMOVAL/INSTALLATION

id091400801400

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the front inner handle. (See INNER HANDLE REMOVAL/INSTALLATION.)

5. Remove the screws, then remove the door lock switch.

ac9uuw00001156

6. Install in the reverse order of removal.