ANTENNA FEEDER NO.1 INSPECTION

id092000812400

With Audio System/Car-navigation System (without display)

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (2) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (3) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Audio unit (See AUDIO UNIT REMOVAL/INSTALLATION.)

  (7) Front scuff plate inner (RH) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (8) Front side trim (RH) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

3. Disconnect the antenna feeder No.2. (See ANTENNA FEEDER NO.2 REMOVAL/INSTALLATION.)

4. Verify that the continuity between antenna feeder No.1 terminals is as indicated in the table.

ac9wzw00002762

  • If not as indicated in the table, replace antenna feeder No.1.

ac9wzw00000898

With Car-navigation System (with display)

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (2) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (3) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Car-navigation unit (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

  (6) Front scuff plate inner (RH) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (7) Front side trim (RH) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

3. Disconnect the antenna feeder No.2. (See ANTENNA FEEDER NO.2 REMOVAL/INSTALLATION.)

4. Verify that the continuity between antenna feeder No.1 terminals is as indicated in the table.

ac9wzw00002862

  • If not as indicated in the table, replace antenna feeder No.1.

ac9wzw00000898