JOINT SHAFT ASSEMBLY [2WD]

id0313008011a3

1. Assemble in the order indicated in the table.

ac9wzw00001447

1 | Bearing housing
2 | Bearing (See Bearing Assembly Note.)
3 | Snap ring
4 | Dust seal (differential side) (See Dust Seal (Differential Side) Assembly Note.)
5 | Joint shaft (See Joint Shaft Assembly Note.)
6 | Snap ring
7 | Dust seal (axle side) (See Dust Seal (Axle Side) Assembly Note.)
8 | Cover

Bearing Assembly Note

1. Install the new bearing using a press and the SST.

ac9uuw00001409

Dust Seal (Differential Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the dust seal (differential side) using a press and the SSTs.

ac9uuw00001410

Joint Shaft Assembly Note

1. Install the joint shaft using a press and the SST.

ac9uuw00001411

Dust Seal (Axle Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the dust seal (axle side) using a press and the SST.

ac9uuw00001412