ON-BOARD DIAGNOSTIC SYSTEM EXTERNAL DIAGNOSTIC UNIT COMMUNICATION FUNCTION [MZI-3.7]

id0102d2141800

Features

• The data link connector 2 (DLC-2) conforming to International Organization for Standardization (ISO) standards has been added.

ac9wzn00000649

DLC-2

  • Shape and terminal arrangement as stipulated by the ISO 15031-3 (SAE J1962) international standard has been adopted. A 16-pin terminal structure is used.

ac9wzn00000650

Terminal | Function
--- | ---
B+ | Battery power supply terminal
CAN_L | Serial communication Lo terminal
CAN_H | Serial communication Hi terminal
GND1 | Body GND terminal
GND2 | Serial communication GND terminal