THEFT-DETERRENT SIREN FUNCTION [WITH INTRUDER SENSOR]

id0914001155b7

• The theft-deterrent siren is located on the rear, right side of the inside of the trunk side box.
• Controlled by the following vehicle conditions:

  ― Standard alert control
  ― Open circuit alert control

Standard Alert Control

• The siren beeps when receiving an alert initialization signal from the theft-deterrent control module. When a go-to-initial signal is received the siren is stopped.

am2zzn00000754

Open Circuit Alert Control

• A back-up power supply is integrated in the theft-deterrent siren.
• When an open circuit is detected in the related wiring harness, the theft-deterrent siren beeps using the back-up power supply.
• If any one of the following conditions are met, the siren is stopped:

  ― Receives go-to-initial signal from the theft-deterrent control module.

am2zzn00000772