REAR DOOR REMOVAL/INSTALLATION

id091100520600

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

ac9uuw00003064

1 | Connector
2 | Bolt A
3 | Bolt B
4 | Rear door

3. Install in the reverse order of removal.

4. Adjust the front door. (See DOOR ADJUSTMENT.)

Connector Removal Note

1. While pressing the tab in the direction of arrow (1), disconnect the connector in the direction of arrow (2).

am6zzw00001397