REAR FENDER PANEL INSTALLATION [PANEL REPLACEMENT]

id098008745000

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for the plug welding before installing the new parts.

3. Before installing new parts, apply spot weld sealer to the tire arch line.

  Note
  • Spot weld sealer is spread on the arrow part of the figure.

4. After temporarily installing new parts, make sure the related parts fit properly.

5. Install the rear fender panel.

ac9wzb00000009