POWER LIFTGATE (PLG) REAR SWITCH INSPECTION

id091100001800

1. Verify that the continuity between the PLG rear switch terminals is as indicated in the table.

ac9uuw00000857

  • If not as indicated in the table, replace the PLG rear switch.

  ac9uuw00000858

2. Apply battery voltage to PLG rear switch terminal A, and connect terminal B to ground.

3. Verify that the LED illuminates.

  • If there is any malfunction, replace the PLG rear switch.