FRONT SIDE FRAME COMPONENT INSTALLATION [PANEL REPLACEMENT]

id098008742000

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for the plug welding before installing the new parts.

3. To prepare for installation, drill 2 through holes at the locations indicated by (A).

4. Weld the 2 locations indicated by (B) from the interior.

am8rrb00000036

5. After temporarily installing new parts, make sure the related parts fit properly.

6. Weld the remaining weld locations and install the front side frame component.

ac9uub00000092