CLEARING DTC [AUDIO]

id0902f6855600

  Caution
  • Before clearing the memory, be sure to enter all of the DTCs displayed in the on-board diagnostic test mode in the Audio Repair Order Form.

1. Launch the on-board diagnostic test mode. (See STARTING PROCEDURE FOR ON-BOARD DIAGNOSTIC TEST MODE [AUDIO].)

2. While pressing the POWER/VOLUME switch, simultaneously press the AUDIO CONT/TUNE switch for 2 s or more.

With RDS (radio data system)

amxzzw00002454

Without RDS (radio data system)

amxzzw00002455

3. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.