POWER RETRACTABLE HARDTOP SWITCH INSPECTION

id091600811700

1. Verify that the continuity between the power retractable hardtop switch terminals is as indicated in the table.

e5e916zw6011

  • If not as indicated in the table, replace the hazard warning switch.

2. Apply battery voltage to power retractable hardtop switch terminal L, and connect terminal C to ground.

e5e916zw6012

3. Verify that the LED illuminates.

  • If there is any malfunction, replace the hazard warning switch.