FUEL INJECTION CONTROL OUTLINE [L8, LF]

id0140i7101700

• Performs optimum fuel injection according to engine operation conditions.
• The PCM determines the engine operation conditions based on the signals from the following input devices and drives the injectors at the optimum fuel injection time (fuel injection amount) and the fuel injection timing to inject fuel. For the construction/operation of the fuel injector, refer to “FUEL SYSTEM, FUEL INJECTOR CONSTRUCTION/OPERATION”.