SIDE WALL REMOVAL/INSTALLATION

id091700454400

  Caution
  • Do not pull the side wall ends outward to remove the side wall. The side wall and clips could be damaged.

  Note
  • The removal procedure is the same for the driver’s side.

1. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

2. Remove the screws.

amxzzw00001404

3. Detach hook A, tab B, D and clip C while pulling the side wall.

amxzzw00001405

4. Remove the side wall.

5. Install in the reverse order of removal.