NO.10 FREQUENT SHIFTING [SJ6A-EL]

id050307801500

10 | Frequent shifting
DESCRIPTION | • Downshifting occurs suddenly even when accelerator pedal is depressed slightly in D range.
POSSIBLE CAUSE | • The malfunctioning circuit is basically the same as “NO.9 ABNORMAL SHIFTING”. (See NO.9 ABNORMAL SHIFTING [SJ6A-EL].) However, a malfunction of the input signal to the APP sensor, TP sensor, turbine sensor, VSS (including the sensor GND, sensor wiring harness and connector), or clutch slippage (clutch stuck, low pressure in line) may also be the cause.