SOLENOID VALVE INSPECTION [SJ6A-EL]

id051311253200

  Caution
  • Water or foreign material entering the connector can cause poor connections or corrosion. Be sure that water or foreign material do not enter the connector when disconnecting it.
  • Do not damage the terminals.

Resistance inspection (On-vehicle)

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the coupler component connector.

amxzzw00000771

4. Measure the resistance between the following terminals.

amxzzw00000147

  • If there is any malfunction, inspect the coupler component.

  • If the coupler component is normal, replace the control valve body. (See CONTROL VALVE BODY REMOVAL [SJ6A-EL].) (See CONTROL VALVE BODY INSTALLATION [SJ6A-EL].)

Solenoid valve resistance (ATF temperature: 20 °C {68 °F})

Terminals | Solenoid valve | Resistance (ohm)
--- | --- | ---
O—GND | Shift solenoid A | 11—15
N—GND | Shift solenoid B | 11—15
M—GND | Shift solenoid C | 11—15
L—GND | Shift solenoid D | 11—15
K—GND | Shift solenoid E | 11—15
E—F | Shift solenoid F | 5.0—5.6
C—D | Shift solenoid G | 5.0—5.6
I—J | Line pressure control solenoid | 5.0—5.6
G—H | TCC control solenoid | 5.0—5.6

5. Connect the coupler component connector.

6. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

7. Install the battery cover.

Continuity Inspection (On-Vehicle Inspection)

  Caution
  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to allow water or foreign material on the connector when disconnecting.
  • Do not damage the terminals.

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the coupler component connector.

amxzzw00000771

4. Verify that there is no continuity between coupler component terminals C, D, E, F, G, H, I, J and GND.

  • If there is any malfunction, inspect the coupler component.

  • If the coupler component is normal, replace the control valve body. (See CONTROL VALVE BODY REMOVAL [SJ6A-EL].) (See CONTROL VALVE BODY INSTALLATION [SJ6A-EL].)

5. Connect the coupler component connector.

6. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

7. Install the battery cover.