NEUTRAL SWITCH REMOVAL/INSTALLATION [M15M-D]

id051110247100

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the transmission. (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].)

4. Remove the neutral switch.

amxzzw00000492

5. Install the neutral switch and a new packing to the transmission case.

  Tightening torque

  25—34 N·m
  {2.6—3.4 kgf·m, 19—25 ft·lbf}

6. Install the transmission. (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].)