STEERING GEAR AND LINKAGE CONSTRUCTION

id061400100600

• A size and weight reduced rack and pinion system steering gear has been adopted.
• Heightened support rigidity has been achieved due to the integration of the steering gear mounts (two locations) and gear housing, improving response and steering stability.
• A check valve equipped to the power steering fluid intake port prevents the power steering fluid from flowing back as a result of road surface resistance. Due to this, kickback from the road surface is reduced.

d5e614zt6002