MANUAL MODE SHIFT CONTROL OPERATION [SJ6A-EL]

id051311326200

Manual Mode Shift

• When the selector lever is shifted over from the D to M range position, the M range switch in the selector lever component turns on, sending a manual mode command signal to the TCM which activates the manual mode shift control.
• When in manual mode and the selector lever is operated in the back (+) direction, the up switch in the selector lever component is turned on and an up-shift command signal is input to the TCM.

  ― The TCM, triggered by the up-shift command signal, carries out shifting by outputting an operation signal to the shift control solenoid.

• Conversely, when the selector lever is operated in the forward (-) direction, the down switch in the selector lever component turns on, and a down-shift command signal is input to the TCM.

  ― The TCM, triggered by the down-shift command signal, carries out shifting by outputting an operation signal to the shift control solenoid if the vehicle speed is less than the set speed and the gear position is 2GR or above.

• The up/down operation of the steering shift switch is the same as the manual operation of the selector lever.
• The TCM utilizes a specialized M range automatic shift diagram. Due to this, restriction of manual shift demand and automatic control of downshifting is carried out, reducing load on the AT, preventing engine over-rev and ensuring drive stability.
• If the vehicle speed exceeds the set speed for each gear while driving in the M range, shift-up is performed automatically so that the vehicle does not lose acceleration.

Condition | Shift control | Note
--- | --- | ---
1GR→2GR up-shift command, at low speed | • To reduce load on the AT, upshifting is inhibited until vehicle reaches speed possible for upshifting | —
2GR→3GR up-shift command, at low speed
3GR→4GR up-shift command, at low speed
4GR→5GR up-shift command, at low speed
5GR→6GR up-shift command, at low speed
5GR→6GR up-shift command, low ECT | • To rapid engine warming-up, upshifting to 6GR is inhibited
6GR→5GR down-shift command, above set speed | • To prevent engine over-rev, downshifting is inhibited until vehicle reaches speed possible for downshifting | • Gear position indicator light flash to alert driver
5GR→4GR down-shift command, above set speed
4GR→3GR down-shift command, above set speed
3GR→2GR down-shift command, above set speed
2GR→1GR down-shift command, above set speed
In 6GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure drive stability, automatically downshifts from 6GR to 5GR | —
In 5GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure drive stability, automatically downshifts from 5GR to 4GR
In 4GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure drive stability, automatically downshifts from 4GR to 3GR
In 3GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure drive stability, automatically downshifts from 3GR to 2GR
In 2GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure drive stability, automatically downshifts from 2GR to 1GR
Wide open throttle at 175—210 km/h {109—130 mph} in 6GR | • To improve acceleration performance, 6GR to 5GR kickdown occurs | —
Wide open throttle at 40—174 km/h {25—108 mph} in 5GR | • To improve acceleration performance, 5GR to 4GR kickdown occurs

Shift Diagram

amxzzn00000270