DOOR HINGE REMOVAL/INSTALLATION

id091100620900

1. Disconnect the negative battery cable.(SeeBATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION.)

  (2) Front combination lights (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

  (3) Side step molding (See SIDE STEP MOLDING REMOVAL.) (See SIDE STEP MOLDING INSTALLATION.)

  (4) Front fender panel (See FRONT FENDER PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

amxzzw00000218

1 | Bolt
2 | Door hinge

4. Install in the reverse order of removal.

5. Adjust the door. (See DOOR ADJUSTMENT.)