NO.5 DSC*2 OPERATES FREQUENTLY/DSC DOES NOT WORK CORRECTLY *2: DSC INDICATOR LIGHT GOES ON AND OFF WHILE DSC IS OPERATING [DYNAMIC STABILITY CONTROL (DSC)]

id0403b2803500

5 | DSC*2 operates frequently/ DSC does not work correctly *2: DSC indicator light goes on and off while DSC is operating
--- | ---
POSSIBLE CAUSE | • DSC HU/CM DTC is stored (input and output device malfunction) • Poor installation of combined sensor and/or steering angle sensor (DSC operates intermittently) • DSC HU/CM, combined sensor or steering angle sensor initialization is not performed after replacement (DSC does not work correctly)

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT DSC HU/CM DTC • Perform the Reading DTCs Procedure. (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].) • Are any DTC present? | Yes | Go to the appropriate DTC inspection. (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].)
No | Go to the next step.
2 | INSPECT INSTALLATION OF COMBINED SENSOR AND STEERING ANGLE SENSOR • Inspect the installation of combined sensor and steering angle sensor. • Are the sensors securely installed? | Yes | Go to the next step.
No | Install the combined sensor and steering angle sensor securely.
3 | VERIFY THAT COMBINED SENSOR AND STEERING ANGLE SENSOR IS INITIALIZED • Verify that combined sensor and steering angle sensor was initialized after replacement. • Was the initialization performed? | Yes | Perform the “Intermittent Concern Troubleshooting”. (See PRECAUTION [DYNAMIC STABILITY CONTROL (DSC)].)
No | Perform the initialization procedure. (See COMBINED SENSOR INITIALIZATION PROCEDURE.) (See STEERING ANGLE SENSOR INITIALIZATION PROCEDURE.)