FRONT BUMPER DISASSEMBLY/ASSEMBLY

id091000405200

Vehicles Without Active Bonnet

Type A (Vehicles with power retractable hardtop)

1. To disassemble the front bumper, remove the following parts:

  (1) Front fog lights (Vehicles with front fog light) (See FRONT FOG LIGHT REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

amxzzw00000987

1 | Fastener A
2 | Set plate RH
3 | Set plate CTR
4 | Set plate LH
5 | Fastener B
6 | Energy absorbing form
7 | Front bumper mesh
8 | Front fog light bezel
9 | Front fog light hole cover (Vehicles without front fog light)
10 | Ornament
11 | License plate holder
12 | Front bumper fascia

3. Assemble in the reverse order of disassembly.

Type A (Vehicles without power retractable hardtop)

1. To disassemble the front bumper, remove the following parts:

  (1) Front fog lights (Vehicles with front fog light) (See FRONT FOG LIGHT REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

amxzzw00000988

1 | Fastener A
2 | Set plate RH
3 | Set plate CTR
4 | Set plate LH
5 | Fastener B
6 | Energy absorbing form
7 | Front bumper mesh
8 | Front fog light bezel
9 | Front fog light hole cover (Vehicles without front fog light)
10 | Ornament
11 | License plate holder
12 | Front bumper fascia

3. Assemble in the reverse order of disassembly.

Type B

1. To disassemble the front bumper, remove the following parts:

  (1) Front fog lights (Vehicles with front fog light) (See FRONT FOG LIGHT REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

amxzzw00002705

1 | Fastener A
2 | Set plate RH
3 | Set plate CTR
4 | Set plate LH
5 | Fastener B
6 | Energy absorbing form
7 | Front bumper mesh
8 | Front fog light bezel (Vehicles with front fog light)
9 | Front fog light hole cover (Vehicles without front fog light)
10 | Nut C
11 | Ornament
12 | Front bumper fascia

3. Assemble in the reverse order of disassembly.

Vehicles With Active Bonnet

  Warning
  • After the active bonnet has deployed, always newly replace the parts indicated in the active bonnet service warnings in the section dealing with the active bonnet. If the vehicle is driven without part replacement, the active bonnet may not deploy correctly. (See ACTIVE BONNET SERVICE WARNINGS.)
  • If a front bumper fascia in which splitting or cracking has occurred is repaired and reused, an active bonnet sensor may mis-detect vibrations because the way that vibration was transmitted before the repair will have changed, which could result in the active bonnet not functioning normally. If splitting or cracking has occurred on the front bumper fascia, always replace the front bumper fascia and bumper retainer with new parts.
  • If a front bumper fascia in which bending and dents have occurred is repaired and reused, an active bonnet sensor may mis-detect vibrations because the way that vibration was transmitted before the repair will have changed, which could result in the active bonnet not functioning normally. If bending and dents have occurred on the front bumper fascia, always replace the front bumper fascia and bumper retainer with new parts.

1. To disassemble the front bumper, remove the following parts:

  (1) Front fog lights (Vehicles with front fog light) (See FRONT FOG LIGHT REMOVAL/INSTALLATION.)

2. Disconnect the active bonnet sensor connector. (right, center) (left, center) (See Active Bonnetsensor Connector Disconnect Note.)

amxzzw00002704

3. Disassemble in the order indicated in the table.

amxzzw00002707

1 | Fastener A
2 | Set plate RH
3 | Set plate CTR
4 | Set plate LH
5 | Bolt B
6 | Bumper retainer
7 | Fastener C
8 | Energy absorbing form
9 | Front bumper mesh
10 | Front fog light bezel (Vehicles with front fog light)
11 | Front fog light hole cover (Vehicles without front fog light)
12 | Nut D
13 | Ornament
14 | Front bumper fascia

4. Assemble in the reverse order of disassembly.

Active Bonnetsensor Connector Disconnect Note

1. Press the location shown by the arrow (1) in the figure and slide the connector in the direction of the arrow (2).

2. Using a flathead screwdriver wrapped in protective tape, lift up the connector in the direction shown by the arrow (3) in the figure and disconnect it in the direction shown by the arrow (4).

amxzzw00002706