DTC B00D2:01 [ACTIVE BONNET]

id0802f1824000

DESCRIPTION | Active bonnet warning light malfunction
--- | ---
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the diagnostic procedure. • Active bonnet warning light malfunction detected
POSSIBLE CAUSE | • Active bonnet warning light malfunction

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM DTC INSPECTION FOR INSTRUMENT CLUSTER • Perform the DTC inspection for the instrument cluster using the M-MDS. (See DTC INSPECTION [INSTRUMENT CLUSTER].) • Is the DTC displayed? | Yes | Repair the malfunctioning part according to the applicable DTC troubleshooting. (See DTC TABLE [INSTRUMENT CLUSTER].)
No | Go to the next step.
2 | INSPECT INSTRUMENT CLUSTER • Verify the warning light illumination using the instrument cluster input/output check mode. (See INSTRUMENT CLUSTER INPUT/OUTPUT CHECK MODE.) ― Check code 26 • Does the active bonnet warning illuminate? | Yes | Go to the next step.
No | Replace the instrument cluster. (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.) Go to the next step.
3 | PERFORM DTC INSPECTION FOR ACTIVE BONNET CONTROL MODULE • Clear the DTC for the active bonnet control module using the M-MDS. (See CLEARING DTC [ACTIVE BONNET].) • Perform the active bonnet control module DTC inspection using the M-MDS. (See DTC INSPECTION [ACTIVE BONNET].) • Is the same DTC displayed? | Yes | Replace the active bonnet control module. (See ACTIVE BONNET CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.