KOEO/KOER SELF TEST [L8, LF]

id0102b1801200

  Note
  • Perform a KOER self test while idling.

1. Connect the M-MDS to the DLC‐2.

amxzzw00000606

2. After the vehicle is identified, select the following items from the initial screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select the “Toolbox” tab.
    2. Select “Self Test”.
    3. Select “Modules”.
    4. Select “PCM”.

  • When using the PDS (Pocket PC)
    1. Select “Module Tests”.
    2. Select “PCM”.
    3. Select “Self Test”.

3. Then, select the “KOEO On Demand Self Test” or “KOER On Demand Self Test” and perform procedures according to directions on the M-MDS screen.

4. Verify the DTC according to the directions on the M-MDS screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection.

5. After completion of repairs, clear all DTCs stored in the PCM, while referring to “AFTER REPAIR PROCEDURE“. (See AFTER REPAIR PROCEDURE [L8, LF].)