CLEARING DTC [ACTIVE BONNET]

id0802f1080600

1. Connect the M-MDS (IDS) to the DLC-2.

amxzzw00001765

2. After vehicle identification, select the following from the IDS initialization screen.

  (1) Select “Self Test”.

  (2) Select “Modules”.

  (3) Select “DHS”.

3. Verify the DTC according to the directions on the screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Switch the ignition to LOCK.

6. Switch ignition ON and hold for 5 s or more.

7. Perform the DTC inspection. (See DTC INSPECTION [ACTIVE BONNET].)

8. Verify that no DTCs are displayed.