PURGE SOLENOID VALVE INSPECTION [L8, LF]

id0116a3800900

Airflow Inspection

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the purge solenoid valve without disconnecting the evaporative hose. (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)

4. Verify that the airflow is as indicated in the table.

amxzzw00000832

Measured condition | Continuity between A—B
--- | ---
When voltage is not applied between terminals A and B | No airflow
When voltage is applied between terminals A and B | Airflow detected

  • If not as specified in the table, replace the purge solenoid valve. (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)