HEADLIGHT LEVELING SWITCH REMOVAL/INSTALLATION

id091800464200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the headlight leveling switch. (See Headlight Leveling Switch Removal Note.)

amxzzw00001095

4. Disconnect the connector.

5. Install in the reverse order of removal.

Headlight Leveling Switch Removal Note

1. Reach into the dashboard through the underside of the lower panel and, while pushing on the tabs of the headlight leveling switch, pull it outward.