MAGNETIC CLUTCH DISASSEMBLY/ASSEMBLY [MANUAL AIR CONDITIONER]

id0740a2800400

1. Disassemble in the order indicated in the table.

e5u740zw5010

1 | Bolt (See Bolt Removal/Installation Note.)
2 | Pressure plate
3 | Shim (See Shim Installation Note.)
4 | Snap ring (See Snap Ring Removal/Installation Note.)
5 | A/C compressor pulley (See A/C Compressor Pulley Removal Note.) (See A/C Compressor Pulley Installation Note.)
6 | Snap ring (See Snap Ring Removal/Installation Note.)
7 | Stator (See Stator Installation Note.)
8 | Clamp
9 | A/C compressor body

2. Assemble in the reverse order of disassembly.

3. Adjust the magnetic clutch clearance. (See MAGNETIC CLUTCH ADJUSTMENT [FULL-AUTO AIR CONDITIONER].)

Bolt Removal/Installation Note

1. When removing or installing the bolt, lock the A/C compressor pulley against rotation using the following procedure.

  Caution
  • When connecting the positive battery cable to the magnetic clutch connector, use a cable with a female terminal of the correct size. Otherwise, load will be applied to the male terminal, resulting in deformation or damage, and poor contact. In addition, the positive battery cable could disconnect from the connector resulting in a short circuit.

  (1) Apply battery positive voltage to the magnetic clutch terminal and connect the A/C compressor body to the ground.

  amxuuw00001070

  (2) Wrap the drive belt, which is no longer of use, tightly around the A/C compressor pulley.

  amxuuw00001071

  (3) Hold the drive belt in place with pliers.

  (4) Remove or install the bolt.
    Tightening torque
    11.8—14.7 N·m {1.21—1.49 kgf·m, 8.7—10.8 ft·lbf}

Snap Ring Removal/Installation Note

1. Remove the snap ring using a snap ring pliers.

e5u740zw5024

A/C Compressor Pulley Removal Note

1. Remove the A/C compressor pulley using the SST (49 0839 425C).

amxzzw00000974

  Caution
  • Be careful that the SST (49 0839 425C) tabs do not hang over the stator.

e5u740zw5021

Stator Installation Note

1. Align the positioning pin with the hole of A/C compressor body and insert.

e5u740zw5025

A/C Compressor Pulley Installation Note

1. Install the inner wheel of the pulley using a plastic hammer and SST (49 B018 003) to the compressor.

  Caution
  • If the SST is not properly positioned when the A/C compressor pulley is press-fit, the A/C compressor axle will interfere with the SST, possibly damaging component parts. Verify that the SST and axle are properly positioned and perform the procedure very carefully.

amxzzw00000691

Shim Installation Note

1. First, insert the 1 mm (0.039 in) thick shim into the shaft.

e5u740zw5023