FRONT COMBINATION LIGHT REMOVAL/INSTALLATION

id091800464400

  Warning
  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove the bolt and fastener shown in the figure.

amxzzw00001012

5. Remove the bolt shown in the figure.

amxzzw00001013

6. Remove the bolt shown in the figure.

amxzzw00001014

7. Disconnect the connectors shown in the figure.

amxzzw00001015

8. Remove the front combination light.

9. Install in the reverse order of removal.(See Front Combination Light Installation Note.)

10. Adjust the headlight aiming. (See HEADLIGHT AIMING.)

Front Combination Light Installation Note

  Caution
  • When replacing the front combination light, refer to the following disassembly figure and verify that parts are assembled correctly. If a part has not been assembled correctly, it could cause problems such as water leakage or fogging in the housing.

Halogen type

amxzzw00003901

Discharge type

amxzzw00003902

  Note
  • Parts necessary for assembly vary depending on the vehicle's manufacturing period and specifications.