AIR INTAKE CONTROL OPERATION [FULL-AUTO AIR CONDITIONER]

id0740a1103500

Air Intake Automatic Control

• The climate control unit calculates the air intake actuator angle (air intake mode) based on the target temperature and operates the actuator.

amxzzn00000359

Correction

Defroster correction
• When the airflow mode is turned to the defroster, the air intake is fixed at fresh air intake to improve defrosting.

Air Intake Manual Control

• The air intake mode can be switched by operation of the REC switch.

Air intake mode | REC switch operation
--- | ---
FRESH | Sets to FRESH when REC switch is turned on during REC mode.
REC | Sets to REC when REC switch is turned on during FRESH mode.