FOREWORD [ACTIVE BONNET]

id0803f1000600

• For troubleshooting, follow the troubleshooting procedure after verifying the symptom No. on the symptom troubleshooting chart.
• When performing an asterisked (*) troubleshooting inspection, first verify the damage and connection status of the connectors and terminals, then perform the inspection while shaking the wiring harness to discover whether poor contact points are the cause of an intermittent malfunction. If there is a malfunction in the connectors or terminals, securely connect, repair, or perform replacement.