TRANSMISSION/TRANSAXLE SPECIFICATIONS

id050000100600

Clutch

Item | Specifications
--- | ---
L.H.D. | R.H.D.
Clutch control | Hydraulic
Clutch cover | Spring type | Diaphragm
Set load | (N {kgf, lbf}) | 5,200 {530, 1,169}
Clutch disc | Outer diameter | (mm {in}) | 215 {8.46}
Inner diameter | (mm {in}) | 155 {6.10}
Clutch pedal | Type | Suspended
Pedal ratio | 5.46
Full stroke | (mm {in}) | 130 {5.118} | 131.6 {5.181}
Clutch master cylinder inner diameter | (mm {in}) | 15.87 {0.6248}
Clutch release cylinder inner diameter | (mm {in}) | 19.05 {0.7500}
Clutch fluid type | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT-3 or DOT-4 Australian specs.: SAE J1703, FMVSS 116 DOT-3

Manual Transmission [M15M-D]

Item | Specification
--- | ---
Transmission control | Floor-shift
Shift assist | Synchromesh
Gear ratio | 1st | 3.136
2nd | 1.888
3rd | 1.330
4th | 1.000
5th | 0.814
Reverse | 3.758
Oil | Grade | API Service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Above 10°C {50°F} | SAE 80W-90
Capacity (approx. quantity) | (L {US qt, lmp qt}) | 2.0 {2.1, 1.8}

Manual Transmission [P66M-D]

Item | Specifications
--- | ---
Transmission control | Floor-shift
Shift assist | Synchromesh
Gear ratio | 1st | 3.709
2nd | 2.190
3rd | 1.536
4th | 1.177
5th | 1.000
6th | 0.832
Reverse | 3.603
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Capacity (approx. quantity) | (L {US qt, lmp qt}) | 2.1 {2.2, 1.8}

Manual Transmission Shift Mechanism

Item | Specification
--- | ---
Transmission control | Floor-shift
Operation system | Direct

Automatic Transmission [SJ6A-EL]

Item | Specification
--- | ---
Gear ratio | 1GR | 3.538
2GR | 2.060
3GR | 1.404
4GR | 1.000
5GR | 0.713
6GR | 0.582
Reverse | 3.168
ATF | Type | JWS3309
Capacity (Approx. quantity) (L {US qt, lmp qt}) | 7.4 {7.8, 6.5}
Torque converter stall torque ratio | 2.00
Hydraulic system (Number of drive/driven plates) | C1 clutch | 4/4
C2 clutch | 5/5
C3 clutch | 4/3
C4 clutch | 4/4
B1 brake | 3/3
B2 brake | 4/3
B3 brake | 3/3
B4 brake | 5/4
Front planetary gear (Number of teeth) | Sun gear | 33
Pinion gear (inner) | 19
Pinion gear (outer) | 18
Ring gear | 75
Middle planetary gear (Number of teeth) | Sun gear | 26
Pinion gear | 20
Ring gear | 66
Rear planetary gear (Number of teeth) | Sun gear | 26
Pinion gear | 20
Ring gear | 66

Automatic Transmission Shift Mechanism

Item | Specification
--- | ---
Transmission control | Floor-shift
Operation system | Rod
Selector lever type | Sport AT