BACK TRIM REMOVAL/INSTALLATION

id091700807900

1. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

2. Pull the open hook lever outward and remove it while pinching the tabs as shown in the figure.

e5u917zw5043

3. Remove the fasteners.

amxzzw00001421

4. Pull the back trim outward and detach clips A and B.

5. Remove the back trim.

6. Install in the reverse order of removal.