SUSPENSION SPECIFICATIONS

id020000100300

Suspension

Item | Specification
--- | ---
Vehicle equipped with 16-inch wheel and tire | Vehicle equipped with 17-inch wheel and tire
Front suspension | Type | Double-wishbone
Spring type | Coil spring
Shock absorber type | Monotube type: High-pressure gas charged, cylindrical, double-acting
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | Vehicle with Power Retractable Hardtop: 22.2 {0.87} Vehicle without Power Retractable Hardtop: 21.0 {0.83}
Wheel alignment (Unloaded*) | Total toe-in | Tire [Tolerance ±4 {0.15}] | (mm {in}) | 1.6 {0.063}
Rim inner | 1.1±2.6 {0.04±0.10} | 1.1±2.8 {0.04±0.11}
Degree | 0°09′±22′
Maximum steering angle [Tolerance ±3°] | Inner | 38°42′
Outer | 32°54′
Caster angle (Reference) [Tolerance ±1°] | 5°56′ | 6°04′
Camber angle (Reference) [Tolerance ±1°] | -0°07′ | -0°13′
Steering axis inclination (Reference) | 10°57′ | 11°04′
Rear suspension | Type | Multi-link
Spring type | Coil spring
Shock absorber type | Monotube type: High-pressure gas charged, cylindrical, double-acting
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 11.0 {0.43} | Standard suspension: 11.0 {0.43} Sport suspension: 12.0 {0.47}
Wheel alignment (Unloaded*) | Total toe-in | Tire [Tolerance ±4 {0.15}] | (mm {in}) | 3 {0.12}
Rim inner | 1.8±2.4 {0.071±0.094} | 2.2±2.8 {0.083±0.110}
Degree | 0°17′±22′
Camber angle [Tolerance ±1°] | -1°04′ | -1°11′

* :Unloaded: Fuel tank is full. Engine coolant and engine oil are at specified level. Jack and tools are in designated position.

Wheel and Tire

Item | Specification
--- | ---
Tire | Size | 205/50R16 87V | 205/45R17 84W
Wheel | Size | 16 x 6 1/2JJ | 16 x 6 1/2J | 17 x 7J
Material | Steel | Aluminum alloy
Offset | (mm {in}) | 50 {2.0} | 55 {2.17}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}