OIL CONTROL VALVE (OCV) REMOVAL/INSTALLATION [L8, LF]

id0110a9801300

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the plug hole plate. (See PLUG HOLE PLATE REMOVAL/INSTALLATION [L8, LF].)

4. Remove the ignition coils. (See IGNITION COIL REMOVAL/INSTALLATION [L8, LF].)

5. Remove the CMP sensor. (See CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION [L8, LF].)

6. Remove the OCV connector.

7. Remove the ventilation hose. (See QUICK RELEASE CONNECTOR (EMISSION SYSTEM) REMOVAL/INSTALLATION [L8, LF].)

8. Remove the cylinder head cover. (See TIMING CHAIN REMOVAL/INSTALLATION [L8, LF].)

9. Remove the OCV.

amxzzw00002114

10. Install in the reverse order of removal.