POWER STEERING OIL PUMP DISASSEMBLY/ASSEMBLY

id061400800800

  Note
  • The following procedure is for replacement of the O-ring and oil seal only. Replace the pump component if other repairs are necessary.

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

amxzzw00001859

1 | Power steering oil pump component (See Power Steering Oil Pump Component Disassembly Note.)
2 | Pressure switch component
3 | Pressure pipe fitting
4 | O-ring
5 | Control valve
6 | Spring
7 | Suction pipe
8 | O-ring
9 | Rear pump body (See Rear Pump Body Assembly Note.)
10 | Gasket
11 | Clip
12 | Cam ring (See Cam Ring Assembly Note.)
13 | Rotor
14 | Vane (See Vane Assembly Note.)
15 | Side plate
16 | O-ring
17 | Shaft component
18 | Oil seal (See Oil Seal Assembly Note.)
19 | Front pump body

Power Steering Oil Pump Component Disassembly Note

1. Secure the power pressure oil pump using the SST.

amxzzw00001860

  Caution
  • Use the SST to prevent damage to the pump when securing it in a vise.

Oil Seal Assembly Note

1. Install the oil seal in the front pump body using the SST and plastic hammer.

amxzzw00001861

Vane Assembly Note

1. Place the vanes in the rotor with the rounded edges contacting the cam.

amxzzw00001862

Cam Ring Assembly Note

1. Install the cam ring in the front pump body with the mark facing upward.

amxzzw00001863

Rear Pump Body Assembly Note

1. After installing the rear body, manually turn the shaft to verify that it rotates smoothly.