TRANSMISSION OIL REPLACEMENT [M15M-D]

id051110247900

1. Position the vehicle on level ground.

2. Remove the Insulator (except L8). (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].)

3. Remove the drain plug B with washer.

amxzzw00000497

4. Drain the oil into a container.

5. Wipe the drain plug B clean and apply sealant to the drain plug B threads before installing.

6. Install the drain plug B with new washer.

  Tightening torque

  B: 39—59 N·m {4.0—5.9 kgf·m, 29—42 ft·lbf}

7. Remove the check plug A.

amxzzw00000498

8. Add the specified oil from check plug A port until the level reaches the brim of check plug hole.

  Specified oil grade

  API Service GL-4 or GL-5

  Specified oil viscosity

  All season: SAE 75W-90
  Above 10°C {50°F}: SAE 80W-90

  Capacity (approx. quantity)

  2.0 L {2.1 US qt, 1.8 lmp qt}

9. Install the new check plug A.

amxzzw00000499

  Tightening torque

  A: 25—39 N·m {2.6—3.9 kgf·m, 19—28 ft·lbf}

10. Install the Insulator (except L8). (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].)