NO.25 ENGINE STALLS WHEN DRIVING AT SLOW SPEED OR STOPPING [SJ6A-EL]

id050307803000

25 | Engine stalls when driving at slow speed or stopping
DESCRIPTION | • Engine stalls when the brake pedal is depressed while driving at low speed or stopping.
POSSIBLE CAUSE | • The malfunction is in the engine control system (e.g. Fuel injection control, electronic controlled throttle system) Note • Before following the troubleshooting steps, make sure that the Automatic Transmission On-Board Diagnostic and Automatic Transmission Basic Inspection are conducted. (See BASIC INSPECTION [SJ6A-EL].)

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Perform the symptom troubleshooting “NO.10 LOW IDLE/STALLS DURING DECELERATION”. (See NO.10 LOW IDLE/STALLS DURING DECELERATION [L8, LF].) • Is the engine control system normal? | Yes | Perform the symptom troubleshooting “NO.24 ENGINE STALLS WHEN SHIFTED TO D RANGE, OR IN R POSITION”. (See NO.24 ENGINE STALLS WHEN SHIFTED TO D RANGE, OR IN R POSITION [SJ6A-EL].)
No | Repair or replace the malfunctioning part according to the inspection results.
2 | • Verify test results. ― If normal, return to the diagnostic index to service any additional symptoms. ― If malfunction remains, inspect the related Service Information and perform repair or diagnosis. • If the vehicle is repaired, troubleshooting completed. • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM. (See TCM REMOVAL/INSTALLATION [SJ6A-EL].)